**AV-1900 Firmware Update**

1/ WITH POWER DISCONNECTED Remove lid and bridge these two terminals

A picture containing electronics, circuit

Description automatically generated

A picture containing electronics, circuit

Description automatically generated


2/ Connect PC to RS-232



3/ Turn power to amp on.

4/ Run FlyMCU software.


**1** Select Port



**3** Start

**2** Select Hex file

Success:



5/ Disconnect power. Remove bridge on internal terminals. Fix lid.