
**CHANGE BLUETOOTH DEVICE NAME AND PIN**



1. INSTALL BLUESUITE SOFTWARE   
   Download from <https://visionaudiovisual.com/cs-1900p/> (windows only)
2. PAIR PHONE TO SPEAKERS
3. PRESS AND HOLD SW2 BUTTON Release when Blue LED turns off.
4. CONNECT PC TO SPEAKERS WITH USB CABLE (NOT INCLUDED).
5. RUN PSTool. Select **USB\csr0** port



NOTE: if port is not showing load drivers manually from




*C:\Program Files (x86)\CSR\BlueSuite 2.6.4\drivers*

1. TYPE “NAME” IN FILTER Adjust then select **Set**



1. TYPE “FIX” IN FILTER The current PIN in this example is shown below:

PIN: 0 0 0 0

1. 

Adjust PIN (last digit of each group), then press **Set** and **Reset BC**.