STEP 1: PUT MODULE INTO UPDATE MODE

1. Disconnect power and USBC
2. Plug them in again, and within 3 seconds press and hold buttons 7 and 8:

A screenshot of a cell phone

Description automatically generated

When you hear beep for 3 seconds, it is in update mode.


STEP 2: RUN IAP SOFTWARE

1. Select COM port and baud rate, then select *Connect*
2. Enter the details as below.

Set address as below (VERY important)

Set the .bin file path.

Select *Install*



Alternating flashing red and blue lights indicates success. The device will put itself into normal mode.